Generated by EAGLE CAM Processor 8.7.0

Photoplotter Info File: /Users/doof/Documents/eagle/Diode-Cap filter/outputs/diode-cap-filter.gpi

 Date              : 27/09/2018 23:07
 Plotfile          : /Users/doof/Documents/eagle/Diode-Cap filter/outputs/diode-cap-filter.GTL
 Apertures         : generated: 
 Device            : Gerber RS-274-X photoplotter, coordinate format 2.5 inch

Parameter settings:

 Emulate Apertures : no
 Tolerance Draw  + :  0.00 %
 Tolerance Draw  - :  0.00 %
 Tolerance Flash + :  0.00 %
 Tolerance Flash - :  0.00 %
 Rotate            : no
 Mirror            : no
 Optimize          : yes
 Auto fit          : yes
 OffsetX           : 0inch
 OffsetY           : 0inch

Plotfile Info:

 Coordinate Format : 2.5
 Coordinate Units  : Inch
 Data Mode         : Absolute
 Zero Suppression  : None
 End Of Block      : *

Apertures used:

 Code     Shape     Size                  used

 D10      draw      0.0000inch               4
 D11      rectangle 0.0630inch x 0.0512inch    10
 D12      round     0.0500inch               2
 D13      rectangle 0.0500inch x 0.0579inch     2
 D14      round     0.1181inch               4
 D15      draw      0.1181inch               4
 D16      draw      0.0079inch              82
 D17      round     0.0258inch               3
 D18      draw      0.0394inch               4
 D19      draw      0.0276inch               2
 D20      draw      0.0157inch             111

