<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.0">
<drawing>
<library>
<packages>
<package name="THT_OVAL">
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;
&lt;p&gt;Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140&lt;/p&gt;
&lt;p&gt;SMA is the smallest package in the DO-214 standard (DO-214AC)&lt;/p&gt;</description>
</package>
<package name="SANYO-OSCON_E12">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
</packages>
<symbols>
<symbol name="PAD">
<pin name="P" direction="pas"/>
</symbol>
<symbol name="DIODE*-1">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="CPOL">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="THT_OVAL">
<gates>
<gate name="G$1" symbol="PAD"/>
</gates>
<devices>
<device name="" package="THT_OVAL">
<connects>
<connect gate="G$1" pin="P" pad="1 2 3" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SK34A-DIODE-SHOTTKY">
<gates>
<gate name="G$1" symbol="DIODE*-1"/>
</gates>
<devices>
<device name="" package="SMA-DIODE">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-POL">
<gates>
<gate name="G$1" symbol="CPOL"/>
</gates>
<devices>
<device name="" package="SANYO-OSCON_E12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
